0
Dipole
image001.jpg
The default type, simple dipole element. Default Length = 0.48 Lambda
1
SQuad
image002.jpg
A square quad shape centred on the nominal boom. Driven point mid lower section. Default Length = 0.27 Lambda
2
Folded
image003.jpg
A simple square folded dipole distributed around nominal boom, Voltage source in lower wire. Default Length = 0.42 Lambda, Default VSpace(P1) = 0.075 Lambda
3
2Dipole
image004.jpg
Two identical dipoles one above the other distributed above and below nominal boom. A Passive element only. Default Length = 0.48 Lambda, VSpace(P1) = 0.3 Lambda
4
FoldedFlatF
image005.jpg
Square Folded Dipole laid flat (Horizontal). Driven wire at nominal spacing, other wire towards front of antenna. Nominal Boom through both elements. Default Length = 0.42 Lambda, HSpace(P1) = 0.075 Lambda
5
FoldedFlatB
image006.jpg
Square Folded Dipole laid flat (Horizontal). Driven wire at nominal spacing , other wire towards back of antenna. Nominal Boom through both elements. Default Length = 0.42 Lambda, HSpace(P1) = 0.075 Lambda
6
3Dipole
image007.jpg
Three identical dipoles above each other distributed above and below nominal boom. A Passive element only. Default Length = 0.48 Lambda, VSpace(P1) = 0.25 Lambda
7
4Dipole
image008.jpg
Four identical dipoles above each other distributed above and below nominal boom. A Passive element only. Default Length = 0.48 Lambda, VSpace(P1) = 0.2 Lambda
8
BentDipF
image009.jpg
Dipole with forward bend. In plain of nominal boom. Driven wire at nominal spacing , other wires bent towards front of antenna. Default Length = 0.38Lambda, Bend(P1) = 0.1 Lambda, Inner(P2) = 0.25 Lambda
9
BentDipB
image010.jpg
Dipole with backwards bend. In plain of nominal boom. Driven wire at nominal spacing , other wires bent towards back of antenna. Default Length = 0.38 Lambda, Bend(P1) = 0.1 Lambda, Inner(P2) = 0.25 Lambda
10
BentDipU
image011.jpg
Dipole with Upwards bend. Driven wire at nominal spacing , other wires bent up from antenna. Default Length = 0.38 Lambda, Bend(P1) = 0.1 Lambda, Inner(P2) = 0.25 Lambda
11
BentDipD
image012.jpg
Dipole with Downwards bend. Driven wire at nominal spacing , other wires bent down from antenna. Default Length = 0.38 Lambda, Bend(P1) = 0.1 Lambda, Inner(P2) = 0.25 Lambda
12
BentX
image013.jpg
X Shaped Dipole with bent arms. Driven wire at nominal spacing, other wires up and down from antenna. Default Length = 0.8 Lambda, Bend(P1) = 0.6 Lambda, Inner(P2) = 0.2 Lambda, Driven wire is fixed at 0.0125 Lambda.
13
RndFolded
image014.jpg
Approx. rounded end folded dipole distributed around nominal boom, Voltage source in lower wire. Default Length = 0.42Lambda, Default VSpace(P1) = 0.058 Lambda, Rad(R) of end circles =P1/2 End segs each 0.765*R
14
RndLoop
image015.jpg
Approx. rounded (Octagonal) loop on nominal boom, Voltage source in lower wire. Default Length = 0.32 Lambda, each octet side is 0.765*Radius
15
VarBowTie
image016.jpg
RSGB Style Skeleton Slot LENGTH=0.19Lambda Middle(P2)= 0.19Lambda Side(P1) = 0.29Lambda, Dual Square Quad LENGTH=0.25Lambda Middle(P2)= 0.25Lambda Side(P1)= 0.25Lambda, VK3DIP Semi-BowTie LENGTH =0.265Lambda Middle(P2)=0.19Lambda Side(P1)= 0.3125Lambda Defaults to VK3DIP Semi-BowTie








